

These two edges must be flat and coplanar.

Sharpening them is like sharpening the back of a chisel. The side of the grinding wheel works best.

If this edge gets rounded over,

Then this side needs to be re-ground to flat.

This edge is the most often sharpened.

This edge is typically not re-ground.

This edge is typically not re-ground.